wdex

WesternDigital7000exSCSIhostadapterdriver

Description

wdex is the device driver for Western Digital 7000ex (EISA bus) SCSI host adapter cards.

In DACB mode, the WD7000ex uses the wdex driver. In ASC mode, the WD7000ex emu - lates the Western Digital WD7000 ISA bus host adapter, and uses the wdha driver.

Before installing the 7000ex, set the card to DACB mode to access its full functionality. Use the EISA configuration utility to change the protocol mode from ASC to DACB.

Refer to the SCO Hardware Compatibility Handbook to determine the support status of your host adapter, or contact your system supplier.

Configuring the wdex driver

You can configure the wdex driver using entries in /etc/conf/cf.d/mdevice and /etc/conf/sdevice.d/wdex. See mdevice(F)and sdevice(F). Changes to these files will only take effect ifthe kernel is relinked using link_unix(ADM) and the machine rebooted.

Con figure wdex driver-specific characteristics by editing the /etc/conf/pack.d/wdex/space.c file.

ioctl commands

The wdex driver supports all standard SCSI ioctls that are defined in the <sys/scsicmd.h> header file and documented on the scsi(HW) manual page.

Diagnostics

See messages(M) for general information about kernel error messages, including a list of generic device driver errors.

Files

/usr/include/sys/scsicmd.h SCSI interface header files

See also

boot(HW), link_unix(ADM), mdevice(F), mkdev(ADM), sconf(ADM), scsi(HW), sde - vice(F)

Chapter 16, ‘‘Adding SCSI host adapters and peripherals ’’in the SCO OpenServer Handbook SCO OpenServer System Administration Guide wdex(AHS)

15 April 1996 1

- -